Jefferson Lab Alignment Group

DATA TRANSMITTAL

TO: J. Gomez, J. LeRose DATE: 2001.10.16 FROM: Kelly Tremblay Checked: # : A711 DETAILS:

The encoder ring for the Hall A spectrometers, was surveyed on October 15, 2001.

Five foil targets were placed on the outer edge of the ring and surveyed using the Hall A survey control points. The five targets were placed on the beam left side from approximately +77° to +168° azimuth from the beamline (right hand rule, following along beam is 0° azimuth). A circle fit was then used to determine the center and radius of the encoder ring.

Relative to Hall�s coordinate system (origin, hall center, positive z along beam, right handed system) the coordinates of the encoder center are :

Z = -0.25 mm X = -0.24 mm

The radius was determined to be 1.007 meters.