DETAILS: _{Data: step2b\HALLA\TARGET\2007\070228A}

Below are the results from the Hall A solid target ladder survey performed Feb 27, 2007. A +X is beam left from ideal target centerline, a +Y is above, and a +Z is downstream. A +pitch is counter clockwise looking from the beam r ight, a +yaw is ccw from above, and a +roll is cw looking from upstream. Values are in m illimeters and degrees.

COMPONENT Z X Y Yaw

Pitch Roll

Solid target ladder dnst face at middle slot:

-5.92 6.00 -0.03 -29.528 -0.71

5 -0.283

Solid target repeat:

-6.03 5.98 -0.13

Jefferson Lab Alignment Group

Data Transmittal

TO: J. Gomez, D. Meekins, J. LeRose DATE: 28 Feb 2007 FROM: J. Dahlberg Checked: # :A1100