Jefferson Lab Alignment Group

DATA TRANSMITTAL

TO: J. P. Chen, J. LeRose DATE: 01 June 2001 FROM: Jim Dahlberg Checked: # : A672 DETAILS:

Below are the results of the Hall A He3 target ladder and compass survey performed on May 10^{th} and 24^{th}, 2001. The numbers shown for the target ladder represent the amount the survey target would have to move (in mm) to be in the ideal location. A negative X is a movement to the beam right, positive Y is up, and positive Z is downstream. The compass measurements are the average of normal and reverse fields.

Target Del Z Del X Del Y

ATGLADE 0.52 0.39 0.67 ATGLADF - 0.18 0.52 0.63 ATGLADG - 0.61 0.24 0.18 ATGLADH 0.54 0.38 0.25 ATGLADI 0.22 0.06 0.88 ATGLADJ - 0.79 0.19 0.76

Compass parallel to beam would have to rotate 0.03deg. ccw to be in ideal position. Compass perpendicular to beam would have to rotate 0.20 deg. cw to be at ideal position.

TARGET LADDER FRAME

Beam Direction E F tt H G

I J

2