Polarized 3He Target Setup

Caltech JLab U. of Kentucky MIT Princeton U. Temple U.

• NMR and EPR techniques for polarization monitoring. • Elastic scattering for current induced depolarization. • Target used successfully in E94-010 and E95-001. • Target length 40 cm, window thickness 0.1 mm.