æ

Experiment E99-117

Analysis for detector PID efficiency • High PID efficiency required for E99-117

– High pion rate π^−/e^−∼ 20 – High A_π−

– ηπ,rej > 10^4 required • Hall A HRS detector PID efficiency

– Oct.28, 2000, gas cerenkov (GC) testrun – Jan. 2001, 2nd layer of pion rejector installed on left arm – Mar.26, 2001, PID analysis using E94104 data

∗ Identify mirror/PMT problem, loose mount, old PMTs etc. ∗ Detector uninstalled and repaired

– Apr.20, 2001, extension of 0.8m GC installed (Rutgers) – May, 2001, two new PMTs installed on left GC – June 5, 2001, Combined pion rejection efficiency 10^{−4} achieved URL:

http://hallaweb.jlab.org/physics/experiments/he3/A1n/index.html#testrun