2ns), TOF difference ± TOF Cut Location(

-100 -50 0 50 100

Neutral/Charged Ratio

0

2

4

6

8

10 Neutral/Charged Ratio as a Function of TOF cut