Controlled Access Checklist.doc -JJL http://hallaweb.jlab.org/news/minutes/checklist.ps

Hall A Controlled Access Checklist

Before Leaving the Hall Always Check:

q Spectrometer entrance window guards removed q Target window guards removed (n/a for Polarized ^3He tgt.) q No obstructions between scattering chamber and spectrometers q No obstructions to spectrometer movement (both arms) q No spectrometer angle camera obstructions (n.b. Check from the side. Do not

crawl under the spectrometer)

q No obvious problems (leaking coolant, pools of standing water, etc.) q Polar crane positioned over entrance beam pipe

If Polarized ^3He target is in operation check:

q Laser Hut "crash button" is pulled out q Yellow beacon on Laser Hut is ON

If work is done in the spectrometer hut check:

q Detectors are in proper configuration (scintillators not rotated out of position,

etc.)

q No loose cables q Doors fully closed

Before calling for "Beam Permit" check (may be done from the counting house):

q No obstructions to spectrometer angle cameras q Magnet power supplies operational (and in remote mode) q Magnet cryogen levels are OK q Target vacuum <1x10^{-4} (n/a for Polarized ^3He tgt.)

Shift leader Name ^∗

(printed)

Signature Date Time

∗ Must always be signed by the shift leader. If the checklist was filled in by someone other than the shift leader, that person should fill in the2^{nd} line.