Beamline

The bench in front of the target has been modified to accomodate the 
change in target position for use with the septum. In addition to the 
existing diagnostic equipment to determine beam position, direction 
and profile information at the target location with existing harps 
(IHA1H04A and 1HA1H04B) and beam position monitors (IPM1H04A and IPM1H04B) 
it now also holds the cavity monitors for the parity experiments which 
gives both position (IPM1H04BH, IPM1H04BV, IPM1H04CH, 
IPM1H04CV) and current (IBC1H04B, IBC1H04C) information as well as an OTR 
(IOR1H04) to give beam profile information at the target location. The correct 
location of these new and existing equipment is given in the Hall A OSP 
(Operation Safety Procedures) document.
