Jefferson Lab Alignment Group

DATA TRANSMITTAL

TO: B. Wojtsekhowski, B. Reitz, D. Meekins, J. LeRose DATE: 15 Feb 2002 FROM: J. Dahlberg Checked: # : A740 DETAILS:

Below are the results of the Hall A target alignment performed on February 14, 2001. The numbers shown are arranged by cell block, and represent the amount the survey target would have to move (in mm) to be in the ideal location. A negative X is a movement to the beam right, positive Y is a movement up, and positive Z is downstream. Note that target 8 was surveyed in the �base� position which accounts for the large Y offset.

Target Del Z Del X Del Y

1 (TOP CRYO) -1.08 0.82 1.96 2 -0.68 0.68 1.98 3 -0.99 0.77 1.87 4 -1.10 0.69 1.88 5 -1.17 0.49 1.83 6 (BOT CRYO) -1.30 0.48 1.84

7 (OPTICS) -1.25 -0.84 1.49 8 (DUMMY) -1.23 -0.17 39.99

REPEATABILITY ON TGT 1 FIDUCIAL A 0.01 -0.03 -0.09