1 Front end side

Three racks to check. All NIM crate have to powered on. Check single rates on the scaler for the total number of triggers, it should be of the order 1.8 KHz.

Rack Crate On ? T1 rate Hz OK? RR1 NIM Ampli Sum Left RR1 NIM Discriminators RR1 NIM Trigger Logic RR2 NIM Ampli Sum Veto RR2 NIM Trigger Logic RR3 NIM Ampli Sum Left RR3 NIM Discriminators RR3 NIM Trigger Logic

2 DAQ side

Rack spectrometer side Fastbus crate.

All cables plugged to patch panel.

Racks other side Camac discriminators VME crate

Rack Crate On ? RR1 CAMAC Left RR2 CAMAC Veto RR2 CAMAC F1 VME TDC RR3 CAMAC Right

3 Things to be checked if something look wrong

3.1 Thresholds

Discriminator Module Value Read out value Veto CAMAC Left ? ? Sums NIM discriminator 50mV 50mV Neutron Nim Discriminator 20mV TDC CAMAC Discrimintor 200mV 2V