Left PMT

Right PMT

Scintillators

Notes :

1. Only single arm trigger is shown. Relevant for GDH and HAPPEX. When we next do coincidence expt, this will be updated. Also must install S2m detector before hypernuclear.

2. The two spectrometers (L and R) are nearly identical. Shown are locations of modules in R-arm but L-arm is similar.

cra 1, sl 2

cra 1, sl 12

Discr.

Discr.

4516 Logic

On the back of 4516 are two outputs corresp. to Logic result (L+R PMTs) “OR”d in groups 1-8 and 9-16 resp. These are “S1” and “S2” signals. S1 S2

S1 and S2 cra 1, sl 7

4516 Logic

Main Trigger

( T1 = R-arm T3 = L-arm )

Trigger Supervisor

cra 1, sl 20 cra 1, sl 21

Delays

cra 1, sl 23

4564 Logic

Cherenk ov“OR” of 10 PMT

Discr.

MLU strobe S1 S2

Cherenkov

MLU programmed to require 2 of 3 from S1,S2,Cher. but be exclusive of main trigger.

T2 (R-arm) T4 (L-arm)

cra 2, sl 9

strobe (“OR” of Right-PMTs of S1,S2 where S2 earlier) Re- timing TM cra 2, sl 6

Gates

for ADCs, TDCs

SINGLE ARM TRIGGER f or HALL A SPECTR OMETERS_{R. Michaels, Apr 2003}

cra 1, sl 9